emco Bau Logo

**emco Bau**

emco TWINGUARD with nylon flor (NF) 12 NF

|  |  |
| --- | --- |
| **Model** | 12 NF |
| **Load** | Heavy |
| **Support chassis** | Nylon-pile rubber |
| **Tread surface** | Robust strips of nylon-pile rubber combined with aluminium scraping profiles. Scraping profiles also available in brass or anodised finishes. |
| **Standard profile clearance approx. (mm)** | 0 mm, closed system |
| **Colours** | grey |
|  | black |
|  | Zebra |
| **Special colours** | Zebra, grey, black |
| **Connection** | High-strength fibres |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |