

**emco Bau**

emco DIPLOMAT Original SPIN®Safe With ribbed carpet insert 22 SPIN/R

|  |  |
| --- | --- |
| **Model** | 22 SPIN/R |
| **Load** | Normal to heavy |
| **Support chassis** | Reinforced support chassis made using rigid aluminium with sound absorbing insulation on the underside |
| **Approx. height (mm)** | 25.9 |
| **Tread surface** | Recessed, robust, weather-proof coarse-fibre ribbed carpet strips (brand-name fibres) for even better dirt removal. Combined with stainless steel tiles for optimum way guidance for the blind in the entrance area. |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Slip resistance** | Slip-resistance of the insert: R11, slip-resistance of the stainless steel tiles: R10 (in accordance with DIN 51130) |
| **Colours** | Anthracite no. 200 |
| **Connection** | Plastic-coated steel cable |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Colour fastness to artificial light ISO 105-B02** | good 6 |
| **Colour fastness to rubbing ISO 105 X12** | good 4 |
| **Colour fastness to water ISO 105 E01** | good 5 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |