

**emco Bau**

emco MARSCHALL Original With ribbed carpet insert and brush strip 522 SRB

|  |  |
| --- | --- |
| **Model** | 522 SRB |
| **Load** | Extremely heavy |
| **Support chassis** | Reinforced support chassis made using rigid aluminium with sound absorbing insulation on the underside |
| **Support chassis colour** | Aluminium as standard. Anodised colours for an additional charge: EV3 gold, C33 mid-bronze, C35 black or C31 stainless steel |
| **Approx. height (mm)** | 22 |
| **Tread surface** | Recessed, robust, weather-proof, ribbed carpet strips, also with brush strips mounted between the profiles. |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Automatic door systems** | Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 |
| **Colours** | Light grey no. 220 |
|  | Anthracite no. 200 |
|  | Red no. 305 |
|  | Brown no. 485 |
|  | Sand no. 430 |
|  | grey |
|  | Black |
| **Flammability** | Insert available on request (surcharge applicable) with fire classification Cfl-s1 according to EN 13501. |
| **Connection** | Plastic-coated steel cable |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Pile material** | 100% PP (polypropylene) |
| **Colour fastness to artificial light ISO 105-B02** | good 6 |
| **Colour fastness to rubbing ISO 105 X12** | good 4 |
| **Colour fastness to water ISO 105 E01** | good 5 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |