

**emco Bau**

emco DIPLOMAT Original With rubber insert and cassette brush 522 TLS GCB

|  |  |
| --- | --- |
| **Model** | 522 TLS GCB |
| **Load** | Normal to heavy |
| **Support chassis** | made of rigid aluminium with sound insulation underlay. In the area of the tactile guidance system, the profiles are laid alternately in two heights. |
| **Approx. height (mm)** | 22 |
| **Tread surface** | Recessed, robust, weather-proof profiled rubber inserts. |
| **Standard profile clearance approx. (mm)** | 3 mm, rubber spacers |
| **Colours** | Bristle bundles in grey |
|  | Bristle bundles in black |
|  | black |
|  | Rubber |
| **Connection** | With threaded rod |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |