emco Bau Logo

**emco Bau**

emco MARSCHALL Premium With Outdoor insert 522 TLS PS Outdoor

|  |  |
| --- | --- |
| **Model** | 522 TLS PS Outdoor |
| **Load** | Extremely heavy |
| **Support chassis** | made of rigid aluminium with sound insulation underlay. In the area of the tactile guidance system, the profiles are laid alternately in two heights. |
| **Approx. height (mm)** | 22 |
| **Tread surface** | The weather-resistant Outdoor insert for noticeably thorough removal of coarse dirt. |
| **Standard profile clearance approx. (mm)** | 3 mm, rubber spacers |
| **Colours** | Anthracite |
|  | Brown |
|  | Red |
| **Connection** | With threaded rod |
| **Warranty** | 5 years guarantee |
| **Pile material** | 100% PA 6 (polyamide) |
| **Colour fastness to artificial light ISO 105-B02** | excellent 7 |
| **Colour fastness to rubbing ISO 105 X12** | good 4-5 |
| **Colour fastness to water ISO 105 E01** | good 4-5 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |