

**emco Bau**

emco DIPLOMAT Original With ribbed carpet insert 522 TLS R

|  |  |
| --- | --- |
| **Model** | 522 TLS R |
| **Load** | Normal to heavy |
| **Support chassis** | made of rigid aluminium with sound insulation underlay. In the area of the tactile guidance system, the profiles are laid alternately in two heights. |
| **Approx. height (mm)** | 22 |
| **Tread surface** | Recessed, robust, weather-proof, ribbed carpet strips. |
| **Standard profile clearance approx. (mm)** | 3 mm, rubber spacers |
| **Colours** | Anthracite no. 200 |
|  | Light grey no. 220 |
| **Connection** | With threaded rod |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Pile material** | 100% PP (polypropylene) |
| **Colour fastness to artificial light ISO 105-B02** | good 6 |
| **Colour fastness to rubbing ISO 105 X12** | good 4 |
| **Colour fastness to water ISO 105 E01** | good 5 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |