emco Bau Logo

**emco Bau**

emco PLAZA With cassette brush 542 SCB

|  |  |
| --- | --- |
| **Model** | 542 SCB |
| **Load** | Exceptionally heavy |
| **Support chassis** | Thick-walled, rigid aluminium with impact sound insulation underlay |
| **Approx. height (mm)** | 42 |
| **Tread surface** | Recessed, robust, weather-proof cassette sections, equipped with brush bundles arranged parallel to one another. Actual mat height: + 1 to 2 mm. |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Colours** | Bristle bundles in grey |
|  | Bristle bundles in black |
| **Flammability** | Complete mat system (for bristle bundles in black) available on request (surcharge applicable) with fire classification Cfl-s1 according to EN 13501. |
| **Connection** | Plastic-coated steel cable |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 Email: bau@emco.de · www.emco-bau.com |