emco Bau Logo

**emco Bau**

emco PLAZA With ribbed carpet insert 542 SR

|  |  |
| --- | --- |
| **Model** | 542 SR |
| **Load** | Exceptionally heavy |
| **Support chassis** | Thick-walled, rigid aluminium with impact sound insulation underlay |
| **Approx. height (mm)** | 42 |
| **Tread surface** | Recessed, robust, weather-proof coarse fibre ribbed carpet strips (brand-name fibres) for even better dirt removal. |
| **Standard profile clearance approx. (mm)** | 5 mm, rubber spacers |
| **Automatic door systems** | Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 |
| **Colours** | Light grey no. 220 |
|  | Anthracite no. 200 |
|  | Red no. 305 |
|  | Brown no. 485 |
|  | Sand no. 430 |
| **Flammability** | Insert for Light Grey and Anthracite ribbed carpet colours available on request (surcharge applicable) with fire classification Cfl-s1 according to EN 13501. |
| **Connection** | Plastic-coated steel cable |
| **Warranty** | 4 year warranty |
|  | Warranty conditions are available at: |
| **Colour fastness to artificial light ISO 105-B02** | good 6 |
| **Colour fastness to rubbing ISO 105 X12** | good 4 |
| **Colour fastness to water ISO 105 E01** | good 5 |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |