emco Bau Logo

**emco Bau**

emco dirt collection well 5517AL

|  |  |
| --- | --- |
| **Model** | 5517AL |
| **Weight (kg/m²)** | 8.7 |
| **Approx. material thickness (mm)** | 3,0 |
| **Structure** | An dirt-collection well unit can consist of either a single-piece well, or multiple wells with different widths and depths that are assembled consecutively in a modular fashion. From a visual and functional perspective, the entrance mat is manufactured in the same size with an edging frame. |
| **Material** | Aluminium, bonded and waterproof, interior completely smooth for easy cleaning. Also available in stainless steel (V2A) on request. |
| **Additional data** | The support for the entrance mat is integrated in the well. |
| **Larger dimensions** | Multiple well units are placed next to each other on site to make a single system. |
| **Drainage system** | This type of well does not have a drainage system |
| **Well overall height** | 20mm |
| **Max. well width, one piece (mm)** | 2800 |
| **Max. well depth, one piece (mm)** | 1300 |
| **Dimensions** | Well width:.........................mm |
|  | Well depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |