

**emco Bau**

emco hygiene mats 601

|  |  |
| --- | --- |
| **Colours** | blue |
|  | Cream |
|  | Yellow |
|  | grey |
|  | Orange |
|  | Red |
| **Description** | Roll-up mat with water drainage on all sides and offering maximum hygiene, for laying on the floor |
| **Material** | Upper and lower bars made from soft PVC, securely bonded. Upper bar also profiled |
|  | Entirely corrosion-free and resistant to chlorine, sea water and spa water. |
| **Approx. height (mm)** | 14.5 mm |
| **Slip resistance** | Non-slip in accordance with DIN 51097, classification C - tested by the "Institut der Säurefliesner-Vereinigung (Säurefliesner consortium) |
| **Service and services** | Dimensioning |
|  | Installation service |
| **Comment** | Note: Hygiene mats are only conditionally suitable for installation underwater! |
| **Standard width (mm)** | 600 mm |
|  | 800 mm |
|  | 1000 mm |
| **Cut** | max. 1200 mm |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |