emco Bau Logo

**emco Bau**

emco swimming pool grates 721/22

|  |  |
| --- | --- |
| **Colours** | Beige - similar to RAL 1001 |
|  | Yellow - similar to RAL 1018 |
|  | Grey - similar to RAL 7001 |
|  | White - similar to RAL 9010 |
| **Special colours** | The majority of special colours (according to RAL or tile sample) are available. |
| **Profile run** | Rigid swimming pool grating with grating bars running parallel to the pool edge |
| **Description** | Swimming pool grating that is robust, solid and pleasant to walk on, which efficiently collects the overflow water at the edge of the pool and provides maximum safety and hygiene. |
| **Material** | High quality, extremely hard-wearing plastic, with UV absorber. |
|  | Entirely corrosion-free and resistant to chlorine, sea water and spa water. |
|  | No need for any metal parts; surface enclosed on all sides to provide maximum hygiene. |
| **Support chassis** | Full profile |
|  | (22 x 10 mm) |
| **Finish** | Flat upper profile surface with safety profile seal (SPS). |
| **Profile spacing:** | < 8 mm in accordance with DIN EN 13451-1 and DIN EN 16582-1 (to prevent areas where fingers could become trapped) |
| **Approx. height (mm)** | 22 mm |
| **Connection** | Fibre-glass reinforced polyester pipes as connection elements |
| **Slip resistance** | Non-slip in accordance with DIN 51097, classification C - tested by the "Institut der Säurefliesner-Vereinigung (Säurefliesner consortium) |
| **Variable grating width (mm)** | 100-300 |
| **Service and services** | Dimensioning |
|  | Installation service |
|  | Repairs |
| **Dimensions** | Grate width:.........................mm (channel width) |
|  | Grate length:.........................mm |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |