

**emco Bau**

emco swimming pool grates 723/25 Design

|  |  |
| --- | --- |
| **Colours** | White - similar to RAL 9010 |
|  | Black – similar to RAL 9005 |
| **Description** | Rigid swimming pool grating with grating bars running at right angles to the pool edge |
| **Material** | High quality, extremely hard-wearing plastic, with UV absorber. |
|  | Entirely corrosion-free and resistant to chlorine, sea water and spa water. |
| **Support chassis** | Full profile |
|  | Upper profile surface incl. recesses in the grating, prepared for the application of tiles on-site (only tiles that satisfy non-slip requirements in wet, barefoot areas in accordance with DIN 51097 must be used). |
|  | Cut-outs underneath for low construction heights. |
| **Finish** | Upper recesses in the plastic for gaps between tiles. |
| **Profile spacing:** | < 8 mm according to DIN EN 16582-1 and DIN EN 13451-1. |
| **Approx. height (mm)** | 25 mm |
| **Connection** | Plastic threaded rod with interim spacers. |
| **Service and services** | Dimensioning |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |