emco Bau Logo

**emco Bau**

emco swimming pool grates Installation frame 780

|  |  |
| --- | --- |
| **Colours** | White - similar to RAL 9010 |
|  | White |
| **Description** | Pre-assembled version with angled profile dimensions of 25 x 28 x 3 mm or 28 x 25 x 3 mm suitable for swimming pool gratings with construction heights of 22 and 25 mm. For straight profiles only. |
| **Material** | Polyester (fibre-glass reinforced) |
|  | The wall anchors and spacer brackets that are required (chrome-nickel steel) are included in the scope of delivery. |
| **Service and services** | Dimensioning |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |