emco Bau Logo

**emco Bau**

Clean-off system for smooth underlay EXACT

|  |  |
| --- | --- |
| **Model** | EXACT |
|  | Non-slip underlay for smooth floors |
| **Special colours** | Yellow |
| **Properties** | Effect with no adhesive |
|  | non-slip, dimensionally stable, absorbs the sound of footsteps, hard-wearing, easy to lay and cut |
| **Function** | The underlay stops the clean-off zone from slipping out of place on nearly all smooth floor surfaces. |
| **Rolls (running metres)** | 30 m |
| **Width (cm)** | 80 cm |
|  | 120 cm |
|  | 180 cm |
| **Material structure** | PES/glass yarn fabric, coated on both sides with special acrylate foam. |
| **Thickness** | Approx. 2 mm |
| **Weight (g/m²)** | approx. 420-450 g/m² |
| **Brand** | emco |
| **Dimensions** | Width:.........................m |
|  | Length:.........................m |
| **Contact** | emco Bautechnik GmbH · Memeler Straße 30 · D-42781 Haan · Germany · Tel.: +49 (0)21 29/34 75 80 · Telefax: +49 (0)21 29/34 75 810 · E-Mail: sauberlauf@emco.de · www.emco-bau.com |