emco Bau Logo

**emco Bau**

emco INOX® LINEO 12

|  |  |
| --- | --- |
| **Model** | LINEO 12 |
|  | Material: chrome-nickel steel (V2A). Suitable for emco Diplomat 512. Profile width 50 mm. Different fonts and special widths available. An additional sheet with a thickness of 1 mm is also inserted beneath the stainless steel profile and riveted to this in areas that cannot be seen; this prevents dirt and debris from being pressed down into the letters. |
| **Approx. material thickness (mm)** | 1,5 |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |