emco Bau Logo

**emco Bau**

emco INOX® LINEO 17

|  |  |
| --- | --- |
| **Model** | LINEO 17 |
|  | Material: Chrome-nickel steel (V2A). Suitable for emco Diplomat 517/522. Profile width 50 mm. Different fonts and several widths available. An additional 1 mm thin sheet is inserted beneath the stainless steel profile and riveted to the areas of it which cannot be seen; this prevents dirt and debris from being pressed down into the letters. |
| **Approx. material thickness (mm)** | 1,5 |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 Email: bau@emco.de · www.emco-bau.com |