emco Bau Logo

**emco Bau**

emco LIMBUS without double ring round brushes Limbus 105

|  |  |
| --- | --- |
| **Model** | Limbus 105 |
| **Material** | High-quality solid rubber, weather-proof and abrasion-proof |
| **Approx. height (mm)** | 10.5 |
| **Tread surface** | Octagonal honeycomb pattern with leading edge at side. Dimensional tolerance +/- 1.5% |
| **Water drainage** | Ribs on the underside combined with open honeycomb bases ensure good water drainage even where the construction height is low |
| **Colours** | Rubber honeycomb mat: black |
| **Double ring brush inserts** | Rubber honeycomb mat: black |
| **Custom mats** | Can be cut to rectangular shapes (only possible without leading edge) |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |