

**emco Bau**

Clean-off system MAXIMUS® Image

|  |  |
| --- | --- |
| **Model** | MAXIMUS® Image |
|  | Creative and image-conscious |
| **Construction** | Tufting-Velours 1/8'' |
| **Pile above substrate** | 100% polyamide |
| **Substrate material** | Polyester fleece |
| **Backing material** | For mat size up to 200 x 500 cm 1.4 mm nitrile rubber backing. From mat size bigger than 200 x 500 cm polyvinyl chloride |
| **Pile weight / fibre weight** | 1000 g/m² |
| **Total weight (g/m²)** | 3410 g/m² |
| **Overall height (mm)** | 9 mm |
| **Combustion/fire behaviour** | Bfl-s1 |
| **Slip resistance** | DS (EN 13893) |
| **Colours** | I10 Lemon |
|  | I20 Yellow |
|  | I30 Yellow/orange |
|  | I40 Orange |
|  | I50 Terracotta |
|  | I60 Red |
|  | I70 Oxide red |
|  | I80 Bordeaux |
|  | I90 Light red |
|  | I100 Cherry |
|  | I110 Purple |
|  | I120 Lilac |
|  | I130 Grape |
|  | I140 Magenta |
|  | I150 Peach |
|  | I160 Royal blue |
|  | I170 Light blue |
|  | I180 Petrol blue |
|  | I190 Emerald green |
|  | I200 Marine blue |
|  | I210 Dark green |
|  | I220 Mint |
|  | I230 Leaf green |
|  | I240 Reed green |
|  | I250 Green |
|  | I260 Brown |
|  | I270 Graphite |
|  | I280 Steel blue |
|  | I290 Light blue |
|  | I300 Silver |
|  | I310 Fawn brown |
|  | I320 Sand |
|  | I330 Chestnut |
|  | I340 Grey beige |
|  | I350 Blue grey |
|  | I360 Light grey |
|  | I370 Grey |
|  | I380 Dark grey |
|  | I390 Black |
|  | I400 White\* |
|  | I410 Steel grey |
|  | I420 Gold |
|  | I430 Salmon pink |
|  | I440 Light green |
|  | I450 Sunset |
| **Colour fastness to artificial light ISO 105-B02** | ≥5 |
| **Colour fastness to rubbing ISO 105 X12** | ≥4 |
| **Colour fastness to water ISO 105 E01** | ≥5 |
| **Supplied as rolls** | Made to measure up to a max. width of 200 cm |
|  | Special dimensions on request |
| **Product characteristics** | Soiling and moisture absorption |
| **Brand** | emco |
| **Dimensions** | Width:.........................m |
|  | Length:.........................m |
| **Contact** | emco Bautechnik GmbH · Memeler Straße 30 · D-42781 Haan · Germany · Tel.: +49 (0)21 29/34 75 80 · Telefax: +49 (0)21 29/34 75 810 · E-Mail: sauberlauf@emco.de · www.emco-bau.com |