emco Bau Logo

**emco Bau**

emco INOX® QUADRO 17

|  |  |
| --- | --- |
| **Model** | QUADRO 17 |
|  | Material: Chromium-nickel steel (V2A). Suitable for emco Diplomat 517/522/517L/522L and emco Marschall 517S/522S/517SL/522SL. Profile width 50 mm Partially with surplus width for optical accents. Individual font types or special widths available. Another 1 mm thick thin sheet is also inserted below the stainless steel profile and riveted to it in the areas that are not visible in order to protect the letters against through-printing. |
| **Approx. material thickness (mm)** | 1,5 |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 Email: bau@emco.de · www.emco-bau.com |