

**emco Bau**

emco STRUCTURA without double ring round brushes Structura 220 FR

|  |  |
| --- | --- |
| **Model** | Structura 220 FR |
| **Material** | High-quality solid rubber, weather-proof and abrasion-proof |
| **Approx. height (mm)** | 22 |
| **Tread surface** | Octagonal honeycomb pattern. Dimensional tolerance +/- 1.5% |
| **Water drainage** | Dimples on the underside combined with open honeycomb bases ensure excellent water drainage |
| **Colours** | Rubber honeycomb mat: black |
| **Double ring brush inserts** | Rubber honeycomb mat: black |
| **Flammability** | Fire behaviour in accordance with European standard Bfl-s1. Tested by the Textiles & Flooring Institute GmbH. |
| **Custom mats** | Bespoke cuts enable practically any dimensions to be accommodated. (Mat sizes up to approx. 2 m² are manufactured with the parts bonded together; larger mat systems are supplied in several parts - with solid rubber connection elements) |
| **Dimensions** | Mat width:.........................mm (bar length) |
|  | Mat depth:.........................mm (walking direction) |
| **Contact** | emco Bautechnik GmbH · Breslauer Straße 34 - 38 · D-49808 Lingen (Ems) · Germany · Phone: +49 (0) 591/9140-500 · Fax: +49 (0) 591/9140-852 · Email: bau@emco.de · www.emco-bau.com |