emco Bau Logo

**emco Bau**

Clean-off system Border profile for finishing cut edges in the case of products with PVC heavy-duty coating EDGE PROFILE

|  |  |
| --- | --- |
| **Model** | EDGE PROFILE |
|  | Border profile for finishing cut edges in the case of products with PVC heavy-duty coating |
| **Rolls (running metres)** | 25 m |
| **Brand** | emco |
| **Contact** | emco Bautechnik GmbH · Memeler Straße 30 · D-42781 Haan · Germany · Tel.: +49 (0)21 29/34 75 80 · Telefax: +49 (0)21 29/34 75 810 · E-Mail: sauberlauf@emco.de · www.emco-bau.com |